
Fairburn Parish Council
Lorry Watch Scheme – Reporting Form

	Date:
	Time:

	Road:

	Direction of Travel:

	Registration Number:

	Do you have a photo?      [     ]                   Do you have video?       [     ]

	Description of vehicle, tick all that apply:
	2 axle single       [     ]	Tanker                     [     ]
	2 axle double      [     ]	Curtain sided           [     ]
	3 axle                 [     ]	Livestock carrier      [     ]
	4 axle                 [     ]	Box sided                [     ]
	5 axle                 [     ]	Flat beds.                [     ]
	6 axle                 [     ]	Refrigeration unit    [     ]
	Tipper                 [     ]	Skips                       [     ]

	Colour and any other features: 

	Name or writing on vehicle:

	Any visible load:

	Any other detail which you think might be useful:

	Name of resident:

	Email:

	Mobile:

	Signature, if printed:	Date:


Please email the form to fairburnlorrywatch@gmail.com along with photos or video Personal Information will not be disclosed with your permission.[image: Picture 1]
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